Design Document: Functional Simulator for Subset of ARM instruction set

The document describes the design aspect of myARMSim, a functional simulator for subset of ARM instruction set.

# Input/Output

## Input

Input to the simulator is MEM file that contains the encoded instruction and the corresponding address at which instruction is supposed to be stored, separated by space. For example:

0x0 0xE3A0200A

0x4 0xE3A03002

0x8 0xE0821003

## Functional Behavior and output

The simulator reads the instruction from instruction memory, decodes the instruction, read the register, execute the operation, and write back to the register file. The instruction set supported is same as given in the lecture notes.

The execution of instruction continues till it reaches instruction “swi 0x11”. In other words as soon as instruction reads “0xEF000011”, simulator stops and writes the updated memory contents on to a memory text file.

The simulator also prints messages for each stage, for example for the third instruction above following messages are printed.

* Fetch prints:
  + “FETCH:Fetch instruction 0xE3A0200A from address 0x0”
* Decode
  + “DECODE: Operation is ADD, first operand R2, Second operand R3, destination register R1”
  + “DECODE: Read registers R2 = 10, R3 = 2”
* Execute
  + “EXECUTE: ADD 10 and 2”
* Memory
  + “MEMORY:No memory operation”
* Writeback
  + “WRITEBACK: write 12 to R1”

# Design of Simulator

## Data structure

Registers, memories, intermediate output for each stage of instruction execution are declared as global static. Being static, the variables are not visible outside the file, thus, make the data encapsulated in the myARMSim.h.

* R[16] : 16 registers to process the instructions. Each register is a signed long integer 64 bits.
* MEM\_INST[4000] : Main instruction memory where the the instructions are loaded. Each block is 8 bits (unsigned).
* MEM\_HEAP[4000] : Heap memory for dynamic allocation. Each block is 8 bits (signed).

## Simulator flow:

The simulator executes a program in 2 steps:

1. Memory is loaded with input memory file

Files:

init\_memory.c

load\_program\_memory.c

Functions:

* init\_memory(): initializes all armsim variables to 0
* load\_program\_memory(): reads the .mem input file and loads the instructions into instruction memory

1. Simulator executes instruction one by one.

Simulator executes the instruction till it reaches end of Program Counter (PC) or if it encounters an SWI 0x11 interrupt.

The simulator repeatedly calls fetch, decode, execute, memory and writeback while updating the PC and executes the instructions one by one.

Next we describe the implementation of fetch, decode, execute, memory, and write-back function.

FETCH

Files:

fetch.c

readword.c

Work flow:

1. fetch() : fetches the current instruction word by calling read\_word()
2. readword() : returns the current instruction word by fetching the instruction from memory corresponding to the current value of PC

# Test plan

We test the simulator with following assembly programs:

* Fibonacci Program
* Sum of the array of N elements. Initialize an array in first loop with each element equal to its index. In second loop find the sum of this array, and store the result at Arr[N].